#
# sysstat.ioconf
#
#  Copyright (C) 2004, Red Hat, Inc.
#
#  Maintained by Sebastien Godard (sysstat [at] orange.fr)
#
#  This file gives iostat and sadc a clue about how to find whole
#   disk devices in /proc/partitions and /proc/diskstats
#  Authoritative source is: linux/Documentation/devices.txt
#
# line format, general record:
#   major:name:ctrlpre:ctrlno:devfmt:devcnt:partpre:partcnt:description
#
#  major:		major # for device
#  name:		base of device name
#  ctrlpre:		string to use in generating controller designators
#			 eg: the c in c0d2p6, decimal formatting implied
#			'*' means none or irrelevant
#			'x': exception... record contains a specific name
#                       for a specific minor #, stored in the ctrlno field
#  ctrlno:		which controller of this type is this
#  devfmt:		type of device naming convention
#	a:		alpha: xxa, xxb, ... xxaa, xxab, ... xxzz
#	%string:	string to use in generating drive designators,
#			 eg: the 'd' in c0d2p6 , decimal formatting implied
#	d:		no special translations (decimal formatting)
#  devcnt:		how many whole devs per major number
#  partpre:         	appended to whole dev before part designator
#                        eg. the p in c0d2p6, decimal formatting implied
#			 '*' means none
#  partcnt:		number of partitions per volume
#			 or minor # for exception records
#  description:		informative text
#
# line format, indirect record:
#   major:base_major:ctrlno[:[desc]]
#
#  major:		major number of the device
#  base_major:		major number of the template for this type,
#			 0 for not supported
#  ctrlno:		controller number of this type
#  desc:		controller-specific description
#			if absent the desc from base_major will be
#			 used in sprintf( buf, desc, ctrlno )


1:ram:*:0:d:256:*:1:RAM disks (ram0..ram255)
1:initrd:x:250:d:256:*:1:Initial RAM Disk (initrd)

#2:0:0:Floppy Devices
2:fd:*:0:d:4:*:1:Floppy Devices fd0,fd1,fd2,fd3

3:hd:*:0:a:2:*:64:IDE - Controller %d
22:3:1:
33:3:2:
34:3:3:
56:3:4:
57:3:5:
88:3:6:
89:3:7:
90:3:8:
91:3:9:

#4:0:0:NODEV
#5:0:0:NODEV
#6:0:0:NODEV
7:loop:*:0:d:256:*:1:Loop Devices 

8:sd:*:0:a:16:*:16:SCSI - Controller %d
65:8:1:
66:8:2:
67:8:3:
68:8:4:
69:8:5:
70:8:6:
71:8:7:
128:8:8:
129:8:9:
130:8:10:
131:8:11:
132:8:12:
133:8:13:
134:8:14:
135:8:15:

9:md:*:0:d:256:*:1:Metadisk (Software RAID) devices  (md0..md255)

#10:0:0:NODEV

#11:sr:*:0:d:256:*:1:CDROM - CDROM (sr0..sr255) (deprecated)
11:scd:*:0:d:256:*:1:CDROM - CDROM (scd0..scd255)

#12:0:0:MSCDEX CD-ROM Callback

13:xd:*:0:a:2:*:64:8-bit MFM/RLL/IDE controller (xda, xdb)

#14:0:0:BIOS Hard Drive Callback
#15:0:0:CDROM - Sony CDU-31A/CDU-33A
#16:0:0:CDROM - Goldstar
#17:0:0:CDROM - Optics Storage
#18:0:0:CDROM - Sanyo

19:double:*:0:d:256:*:1:Compressed Disk (double0..double255)

#20:0:0:CDROM - Hitachi

21:mfm:*:0:a:2:*:64:Acorn MFM Hard Drive (mfma, mfmb)

# 22: see IDE, dev 3

#23:0:0:CDROM - Mistumi Proprietary
#24:0:0:CDROM - Sony CDU-535
#25:0:0:CDROM - Matsushita (Panasonic/Soundblaster) #1
#26:0:1:CDROM - Matsushita (Panasonic/Soundblaster) #2
#27:0:2:CDROM - Matsushita (Panasonic/Soundblaster) #3
#28:0:3:CDROM - Matsushita (Panasonic/Soundblaster) #4
# 28:0:0:! ACSI (Atari) Disk Not Supported
#29:0:0:CDROM - Aztech/Orchid/Okano/Wearnes
#30:0:0:CDROM - Philips LMS CM-205
#31:0:0:ROM/flash Memory Card
#32:0:0:CDROM -  Phillips LMS CM-206

# 33: See IDE, dev 3
# 34: See IDE, dev 3

#35:0:0:Slow Memory RAM Disk

36:ed:*:0:a:2:*:64:MCA ESDI Hard Disk (eda, edb)

#37:0:0:Zorro II Ram Disk
#38:0:0:Reserved For Linux/AP+
#39:0:0:Reserved For Linux/AP+
#40:0:0:Syquest EZ135 Parallel Port Drive
#41:0:0:CDROM -  MicroSolutions Parallel Port BackPack
#42:0:0:For DEMO Use Only

43:nb:*:0:d:256:*:1:Network Block devices (nb0..nb255)
44:ftl:*:0:a:16:*:16:Flash Translation Layer (ftla..ftlp)
45:pd:*:0:a:4:*:16:Parallel Port IDE (pda..pdd)

#46:0:0:CDROM - Parallel Port ATAPI

47:pf:*:0:d:256:*:1:Parallel Port ATAPI Disk Devices (pf0..pf255)

48:rd:/c:0:%d:32:p:8:Mylex DAC960 RAID, Controller %d
49:48:1:
50:48:2:
51:48:3:
52:48:4:
53:48:5:
54:48:6:
55:48:7:
136:48:8:
137:48:9:
138:48:10:
139:48:11:
140:48:12:
141:48:13:
142:48:14:
143:48:15:

# 56, 57: see IDE, dev 3:

58:lvm:*:0:d:256:*:1:Logical Volume Manager (lvm0..lvm255)

#59:0:0:PDA Filesystem Device
#60:0:0:Local/Experimental Use
#61:0:0:Local/Experimental Use
#62:0:0:Local/Experimental Use
#63:0:0:Local/Experimental Use
#64:0:0:NODEV

# 65..71: See SCSI, dev 8:

72:ida/:c:0:%d:16:p:16:Compaq Intelligent Drive Array - Controller %d
73:72:1:
74:72:2:
75:72:3:
76:72:4:
77:72:5:
78:72:6:
79:72:7:

80:i2o/hd:*:0:a:16:*:16:I2O Disk - Controller %d
81:80:1:
82:80:2:
83:80:3:
84:80:4:
85:80:5:
86:80:6:
87:80:7:

# 88..91: see IDE, dev 3:

#92:0:0:PPDD Encrypted Disk
#93:0:0:NAND Flash Translation Layer not supported

94:dasd:*:0:a:64:*:4:IBM S/390 DASD Block Storage (dasda, dasdb, ...)

#95:0:0:IBM S/390 VM/ESA Minidisk
#96:0:0:NODEV
#97:0:0:CD/DVD packed writing devices not supported

98:ubd:*:0:d:256:*:1:User-mode Virtual Block Devices (ubd0..ubd256)

#99:0:0:JavaStation Flash Disk
#100:0:0:NODEV

101:amiraid/ar:*:0:d:16:p:16:AMI HyperDisk RAID (amiraid/ar0 - amiraid/ar15)

#102:0:0:Compressed Block Device
#103:0:0:Audit Block Device

104:cciss:/c:0:%d:16:p:16:HP SA 5xxx/6xxx (cciss) Controller %d
105:104:1:
106:104:2:
107:104:3:
108:104:4:
109:104:5:
110:104:6:
111:104:7:

112:iseries/vd:*:0:a:32:*:8:IBM iSeries Virtual Disk (.../vda - .../vdaf)

#113:0:0:CDROM - IBM iSeries Virtual

# 114..159 NODEV

120:emcpower:*:0:a:16:*:16:EMC PowerPath Unit %d

#160:sx8/:*:0:d:8:p:32:Promise SATA SX8 Unit %d
#161:160:1:
160:carmel/:*:0:d:8:p:32:Carmel 8-port SATA Disks (carmel/0 - carmel/7)
161:160:1:

# 162..198 UNUSED

180:ub:*:0:a:32:p:8:USB block devices

#199:0:0:Veritas Volume Manager (VxVM) Volumes
#200:0:0:NODEV
#201:0:0:Veritas VxVM Dynamic Multipathing Driver

202:xvd:*:0:a:16:p:16:Xen Virtual Block Device

# 203..230: UNUSED

232:emcpower:*:0:a:16:*:16:EMC PowerPath Unit %d
233:232:1:
234:232:2:
235:232:3:
236:232:4:
237:232:5:
238:232:6:
239:232:7:
240:232:8:
241:232:9:
242:232:10:
243:232:11:
244:232:12:
245:232:13:
246:232:14:
247:232:15:

# 240..254: LOCAL/Experimental

256:rfd:*:0:a:16:*:16:Resident Flash Disk Flash Translation Layer (rfda..rfdp)

257:ssfdc:*:0:a:8:*:8:SSFDC Flash Translation Layer filesystem (ssfdca..ssfdch)

258:blockrom:*:0:d:256:*:1:ROM/Flash Read-Only Translation Layer (blockrom0...)

