# -*- mode: sh -*-
#-
# Configuration for the rng-tools-debian initscript

# Set to the input source for random data, leave undefined
# for the initscript to attempt auto-detection.  Set to /dev/null
# for the viapadlock driver.
#HRNGDEVICE=/dev/hwrng
#HRNGDEVICE=/dev/null

# Additional options to send to rngd. See the rngd(8) manpage for
# more information.  Do not specify -r/--rng-device here, use
# HRNGDEVICE for that instead.
#RNGDOPTIONS="--hrng=intelfwh --fill-watermark=90% --feed-interval=1"
#RNGDOPTIONS="--hrng=viakernel --fill-watermark=90% --feed-interval=1"
#RNGDOPTIONS="--hrng=viapadlock --fill-watermark=90% --feed-interval=1"
# For TPM (also add tpm-rng to /etc/initramfs-tools/modules or /etc/modules):
#RNGDOPTIONS="--fill-watermark=90% --feed-interval=1"

# If you need to configure which RNG to use, do it here:
#HRNGSELECT="virtio_rng.0"
# Use this instead of sysfsutils, which starts too late.
