# Last Modified: Sat Jan 20 10:45:05 2018
#include <tunables/global>

/usr/sbin/chronyd flags=(attach_disconnected) {
  #include <abstractions/base>
  #include <abstractions/nameservice>

  # For /run/chrony to be created
  capability chown,

  # Give “root” the ability to read and write the PID file
  capability dac_override,
  capability dac_read_search,

  # Needed to support HW timestamping
  capability net_admin,

  # Needed to allow NTP server sockets to be bound to a privileged port
  capability net_bind_service,

  # Needed to allow an NTP socket to be bound to a device using the
  # SO_BINDTODEVICE socket option on kernels before 5.7
  capability net_raw,

  # Needed to drop privileges
  capability setgid,
  capability setuid,

  # Needed to set the SCHED_FIFO real-time scheduler at the specified priority
  # using the '-P' option
  capability sys_nice,

  # Needed to lock chronyd into RAM
  capability sys_resource,

  # Needed to set the system/real-time clock
  capability sys_time,

  /usr/sbin/chronyd mr,

  /etc/chrony/{,**} r,
  /var/lib/chrony/{,*} rw,
  /var/log/chrony/{,*} rw,
  @{run}/chrony/{,*} rw,
  @{run}/chrony-dhcp/{,*} r,

  # Using the “tempcomp” directive gives chronyd the ability to improve
  # the stability and accuracy of the clock by compensating the temperature
  # changes measured by a sensor close to the oscillator.
  @{sys}/class/hwmon/hwmon[0-9]*/temp[0-9]*_input r,
  @{sys}/devices/virtual/thermal/thermal_zone[0-9]*/hwmon[0-9]*/temp[0-9]*_input r,

  # Support all paths suggested in the man page (LP: #1771028). Assume these
  # are common use cases; others should be set as local include (see below).
  # Configs using a 'chrony.' prefix like the tempcomp config file example
  /etc/chrony.* r,
  # Example gpsd socket is outside @{run}/chrony/
  @{run}/chrony.tty{,*}.sock rw,
  # To sign replies to MS-SNTP clients by the smbd daemon
  /var/lib/samba/ntp_signd/socket rw,

  # rtc
  /etc/adjtime r,
  /dev/rtc{,[0-9]*} rw,

  # gps devices
  /dev/pps[0-9]* rw,
  /dev/ptp[0-9]* rw,

  # Allow reading the chronyd configuration file that timemaster(8) generates
  @{run}/timemaster/chrony.conf r,

  # For use with clocks that report via shared memory (e.g. gpsd),
  # you may need to give ntpd access to all of shared memory, though
  # this can be considered dangerous. See https://launchpad.net/bugs/722815
  # for details. To enable, add this to local/usr.sbin.chronyd:
  #     capability ipc_owner,

  # Site-specific additions and overrides. See local/README for details.
  #include <local/usr.sbin.chronyd>
}
